Folder Structure:
|Light Ventilation Series
	|Long
	|Short

All files are applicable for Trim & Trimless, Light + Ventilation & Light Only

File name structure

Light Ventilation Size BB CCXX FF-xxxmA.IES
----------------- ---- -- ---- -- ---
|	   	  |    |  |    |  |Current setting in mA
|		  |    |  |    |Finish colour
|	  	  |    |  |CCT + CRI
|	  	  |    |Beam angle
|	  	  |Shape/Size
|	  	 
|Family Name

Shape/Size
Long or Short

Beam Angle
15 = 15°
25 = 25°
40 = 40°
60 = 60°

CC
24 = 2400K
27 = 2700K
30 = 3000K
35 = 3500K
40 = 4000K
1830 = Dim 2 Warm 3000K to 1800K

XX
90 = CRI90
97 = CRI97

Finish colour
BA  = Black Anodized
BB  = Brushed Bronze
BG  = Brushed Grey
BN  = Brushed Nickle
BS  = Brushed Steel
CFD = Canon Fusil Dark
CFL = Canon Fusil Light
DB  = Dark Bronze
LB  = Light Bronze
WS  = White Structure

